2 Electroacoustic sound system
2.2 Installation of electroacoustic sound system

Recommendations for perfect installation of electroacoustic sound are, as follows:

1. Always place the speakers in a plane perpendicular to the axis from the center of the listening position ⇒ it helps avoid the signal delay between the two signal sources.

The delay can be observed mainly at higher frequencies. The low frequencies are spread evenly (it is the property of a wavelength).

Correct position of speakers in relation to the listener's position

2. Height and center speakers should be placed at the height of the ears

Higher frequencies have narrow directional characteristic, low frequencies spread in every direction.

Correct positioning of high and center speakers in relation to the listener position

3. Place the microphones beyond the direct reach of the speakers.

Correct position of a microphone with respect to the position of the speakers