Minimum about fuzzy logic
Reasons for fuzzy generalization

Foregoing examples of implementation of the majority function and threshold functions were introduced. Now suppose the goal is to secure the object in a similar way, but with the utilization of sensors, which provide continuous output, for example in the range from 0 V to 10 V, so that the zero value corresponds to a safe condition (risk of fire is zero) and the 10 V value corresponds to absolute certainty of fire (risk of fire is one).