Minimum about fuzzy logic
Output terms

Defuzzification can be also considers to be the opposite of fuzzification. We define course of logical functions for individual terms above the output language variables (e.g. in the meaning of bearing failure risk, action hit voltage, regulation gage or valve displacement, time of action hit duration). These terms could have similar shape and dislocation as with input terms definition – usual triangle, trapeze or curves with smooth course.